Certification Design Category

A (Ocean): Designed for extended voyages where conditions

may exceed wind force 8 on the Beaufort

scale (47 mph and above) and significant wave heights

of 4 meters (13.12 feet) and above, and vessels largely

self-sufficient.

B (Offshore): Designed for offshore voyages where

conditions up to, and including, wind force 8 (39-46

mph) and significant wave heights up to, and including

4 meters (13.12 feet) may be experienced.

C (Inshore): Designed for voyages in coastal waters,

large bays, estuaries, lakes and rivers where conditions

up to, and including, wind force 6 (25-31

mph) and significant wave heights up to, and including,

2 meters (6.56 feet) may be experienced.

D (Sheltered waters): Designed for voyages on small

lakes, rivers and canals where conditions up to, and

including, wind force 4 (13-18 mph) and significant

wave heights up to, and including, 0.5 meters (1.64 feet)

may be experienced.

Your 170 Montauk is design category C

The significant wave height is considered to be the

primary factor for determining design category. Other

parameters (e.g. meteorological) are descriptions of

when these wave heights may be expected to occur.

Refer to page 1-11 for weather information.

The certification plate, as well as “Specifications &

Dimensions” on the following page has the maximum

rated power listed for your boat. DO NOT EXCEED

THIS RATING. The various engine types offered today

are more powerful and require constant maintenance to

stay at optimal performance. It is required of the owner/

operator to read all information regarding safety features,

warning notices and maintenance schedules for continued

safe operation of the engine.

The engine on the 170 Montauk has been tested and

proven to be best suited for general use under normal

conditions and load.

If you are re-powering your Boston Whaler®, you should

pay particular attention to the maximum/minimum

horsepower and maximum safe engine weight load your

Boston Whaler® boat is rated for.

The 170 Montauk is designed for a maximum

outboard engine weight of 410 LBS (185 kg).

It is
